**TECHNICAL SPECIFICATION for price survey**

**Purchase of outdoor exercise equipment**

**Commissioning party:** Municipality of Ropaži, Reg. nr. 90000067986, Institute Street 1a, Ulbroka, Stopiņi Parish, LV-2130

**Location of the site:** Berģi School of Music and Arts, Upesciems, Garkalnes parish, Ropaži municipality, LV-2137

**Contact:** Project Manager Līga Mekša, email: liga.meksa@ropazi.lv, tel. +371 25483904; +37127134698

|  |
| --- |
| **Technical requirements** |
| **N. p.k.** | **Pricing Elements** | **Compliance data** |
| 1. **Exercise equipment designed to strengthen muscle groups of the thighs, hips and buttocks**
 |
| 1. | Number of | 1 |
| 2. | Length | At least 2040 mm |
| 3. | Width | At least 930 mm |
| 4. | Height | At least 1880 mm |
| 5. | Allowable user height | From 140 cm |
| 6. | Allowable user age | From 14 years of age |
| 7. | Installation | Appropriate, mobile platform |
| 8. | Material | Steel with a coating layer of at least 4 mm galvanized (zinc) |
| 9. | Adjustment functions | Load, starting height |
| 10 | Weight of equipment | 100 to 300 kg |
| 11. | Units of adjustable weights | 1. - 90 kg
 |
| 12. | Accessibility of instructions | Instructions for use of the training device and information on the fitness of the training device for muscle groups are viewed on the training device and can be easily found electronically (indications on the device) |
| 13. | Exploitation | Applicable in all seasons |
| 14. | Replacement support for moving parts | Applies to |
| **2.) Exercise equipment designed to strengthen muscle groups of breast, tricepse and shoulder parts** |
| 1. | Number of | 1 |
| 2. | Length | At least 2070 mm |
| 3. | Width | At least 930 mm |
| 4. | Height | At least 870 mm |
| 5. | Allowable user height | From 140 cm |
| 6. | Allowable user age | From 14 years of age |
| 7. | Material | Steel with a coating layer of at least 4 mm galvanized (zinc) |
| 8. | Adjustment functions | Grip width, start height |
| 9. | Weight of equipment | Within 170 to 228 kg |
| 10 | Units of adjustable weights | 15-85 kg |
| 11. | Installation | Appropriate, mobile platform |
| 12. | Accessibility of instructions | Instructions for use of the training device and information on the fitness of the training device for muscle groups are viewed on the training device and can be easily found electronically (indications on the device) |
| 13. | Exploitation | Applicable in all seasons |
| 14. | Replacement support for moving parts | Applies to |
| **Additional requirements** |
| N. p.k. |  |  |
| 1. | Delivery | Price quote for transport to the location of the object |
| 2. | Installation | Price quote for installation at the location of the object |
| 3. | Appropriate graphics and/or 3D visual image attached to the offer | Applies to |
| 4. | Warranty period provided | at least 2 years |
| 5. | Warranty coverage against rust | at least 2 years |
| 6. | Provision for maintenance of goods | 2, 12 and 24 months after installation |
| 7. | Price Spotlight Provision | at least until 31.12.2022. |
| 8. | The applicant | The applicant/service provider is a partnership or legal entity established in the European Economic Area, whose main activity includes the production, supply and/or marketing of goods meeting the specification |
| 9. | Conformity of goods | EU Standard EN16630 |

**Separate instructions:**

**Justification for choice of service supplier:** When pooling tenders, the co-operation agreement will be concluded with the selected tenderer offering the lowest price, excluding VAT, according to all specific requirements

**Pricing indicators**: Including VAT (if applicable), indicating EUR per share of the item.

**Contract execution time:** within 6 weeks from the date of signature of the contract.

**The offer to be submitted:** Project Manager of Municitality of Ropaži Development Department of Property and Investments Līga Mekša in electronic form: in e-mail: liga.meksa@ropazi.lv to **27.09.2022.**